UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_event_umq_ulb_receiver_info_ex_t_stct Struct Reference

Structure that holds UMQ ULB receiver information in an extended form. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap set of flags reserved for future use. Currently set to 0.
lbm_umq_regid_t | registration_id
| The registration ID of the receiver.
lbm_uint_t | assignment_id
| The Assignment ID of the receiver.
lbm_uint_t | application_set_index
| The Application Set Index the receiver is in.
char | receiver [LBM_UMQ_ULB_MAX_RECEIVER_STRLEN]
| The receivers immediate message target string.

## Detailed Description

Structure that holds UMQ ULB receiver information in an extended form.

This structure signals to the source various receiver-oriented events. Delivered as source events LBM_SRC_EVENT_UMQ_ULB_RECEIVER_REGISTRATION_EX, LBM_SRC_EVENT_UMQ_ULB_RECEIVER_DEREGISTRATION_EX, LBM_SRC_EVENT_UMQ_ULB_RECEIVER_READY_EX, and LBM_SRC_EVENT_UMQ_ULB_RECEIVER_TIMEOUT_EX via the callback lbm_src_cb_proc.

See lbm_src_event_umq_ulb_receiver_info_ex_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h