UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_umq_index_info_t_stct Struct Reference

Structure that holds information used for sending and receiving messages with UMQ indices. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating extra information about the index. Zero or more flag bits ORed together: LBM_UMQ_INDEX_FLAG_* (i.e. LBM_UMQ_INDEX_FLAG_NUMERIC)
int | reserved
| UM internal only. DO NOT ACCESS DIRECTLY!
char | index [LBM_UMQ_MAX_INDEX_LEN]
| The index.
size_t | index_len
| The length of the index in bytes.

## Detailed Description

Structure that holds information used for sending and receiving messages with UMQ indices.

A structure used with UM sources and receivers to associated UMQ Indices with messages.

See lbm_umq_index_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h