UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_src_create_ex_info_t Struct Reference

Provides information about a joined transport session when the lbm_rcv_src_notification_create_function_ex_cb callback is invoked. See the option source_notification_function_ex (receiver). More...

`#include <lbm.h>`

## Data Fields
lbm_uint32_t | orig_domain_id
| ID number of the Topic Resolution Domain of the originating source.
lbm_uint32_t | hl_idx
| Hot Link index of DRO (if any) providing this transport session.
char | proxy_source [LBM_MSG_MAX_SOURCE_LEN]
| Source String of source or DRO proxy source (if any) providing this transport session.
int | flags
| Bitmap indicating characteristics of the transport session. Zero or more flag bits ORed together: LBM_SRC_NOTIFICATION_EX_INFO_FLAG_* (i.e. LBM_SRC_NOTIFICATION_EX_INFO_FLAG_HOT_LINK)

## Detailed Description

Provides information about a joined transport session when the lbm_rcv_src_notification_create_function_ex_cb callback is invoked. See the option source_notification_function_ex (receiver).

The documentation for this struct was generated from the following file:

- lbm.h