UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_ume_rcv_recovery_info_ex_func_info_t_stct Struct Reference

Structure that holds information for UMP receiver recovery sequence number info application callbacks. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating which optional fields are used. Zero or more flag bits ORed together: LBM_UME_RCV_RECOVERY_INFO_EX_FLAG_* (i.e. LBM_UME_RCV_RECOVERY_INFO_EX_FLAG_SRC_SID)
lbm_uint_t | low_sequence_number
| Lowest sequence number that the receiver will attempt to recover. May be altered to instruct UMP to recover differently.
lbm_uint_t | low_rxreq_max_sequence_number
| Lowest sequence number that the receiver will attempt to recover (with retransmit request maximum taken into account)
lbm_uint_t | high_sequence_number
| Highest sequence number that the receiver has seen from the source. May not be actual highest sent by source.
void * | source_clientd
| The per-source clientd value for the source set by the lbm_rcv_src_notification_create_function_cb callback.
char | source [LBM_MSG_MAX_SOURCE_LEN]
| The source.
lbm_uint64_t | src_session_id
| The session ID for the source.

## Detailed Description

Structure that holds information for UMP receiver recovery sequence number info application callbacks.

A structure used with UMP receiver recovery sequence number information callbacks to pass in information as well as return low sequence number information.

See also
  lbm_ume_rcv_recovery_info_ex_func_t

See lbm_ume_rcv_recovery_info_ex_func_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h