UM C API 6.17.1

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- Data Structures
- Data Fields

Data Fields
lbm_process_events_info_t_stct Struct Reference

Structure that holds information for the extended Process Events calls. More...

`#include <lbm.h>`

## Data Fields
int | flags
| Bitmap indicating which extended features to enable. Zero or more flag bits ORed together: LBM_PROC_EVENT_EX_FLAG_* (i.e. LBM_PROC_EVENT_EX_FLAG_USER_TIME, LBM_PROC_EVENT_EX_FLAG_NO_MAIN_LOOP_MUTEX)
lbm_timeval_t | time_val
| Current time of day, in form as returned by gettimeofday(). When `flags` has LBM_PROC_EVENT_EX_FLAG_USER_TIME set, the application must set this field prior to calling lbm_context_process_events_ex().

## Detailed Description

Structure that holds information for the extended Process Events calls.

A structure used with Sequential Mode that utilize the extended Process Events calls to pass options. See Extended Context Process Events for more information.

See also
  lbm_context_process_events_ex()

See lbm_process_events_info_t_stct for field definitions.

The documentation for this struct was generated from the following file:

- lbm.h